|  |  |  |  |
| --- | --- | --- | --- |
| **DATE/TIME** | **TEMPERATURE** | **INITIAL** | **CORRECTIVE ACTION?** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |
| --- | --- |
|  | **Temperature Monitoring – Cooler – HUB.TRS.REC.26** |
| **Related Documents Used** | **Temperature Control SOP** |
| **Supplied to:** | **HUB User** |
| **Date:** | **June 1, 2022** |
| **Target Temperature Range** | **2°C to 8°C** |
| **Corrective Action** | **Modify temperature dial; advise HUB Manager/Owner** |